Person(s) Conducting the Survey:

Location:

Date:

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
|  | Swings and Slides | | | |
| Condition | |  | | Recommendation/Additional Info |
| Are swing seats 12-24 inches  from the surface? | | Yes | No |  |
| Are swing seats free of splits, cuts and tears? | | Yes | No |  |
| Are the ends of the S-hooks closed? (thickness of a  dime) | | Yes | No |  |
| Do swings have at least 6 feet of clearance from each end of the framework? | | Yes | No |  |
| Do swing-to-swing and swing-to-support clearance on ‘to-fro’ swings equal or exceed 24 inches? | | Yes | No |  |
| Do swings have at least double the length of the swing clearance front and back? | | Yes | No |  |
| Is the use zone twice the length of the swing chain in  both directions? | | Yes | No |  |
| Are there only two swings per bay? | | Yes | No |  |
| Are swings suspended by chains that are in good  condition? | | Yes | No |  |
| Are all upper connections properly lubricated and in good condition? | | Yes | No |  |

|  |  |  |
| --- | --- | --- |
| Swings and Slides (cont.) | | |
| Condition |  | Recommendation/Additional Info |
| Do tire swings have holes drilled in the bottom for proper drainage and are not worn excessively? | Yes No |  |
| Does clearance between tires and fixed objects equal or exceed 30 inches, plus  the arc of the chain? | Yes No |  |

|  |  |  |  |
| --- | --- | --- | --- |
| Slides | | | |
| Condition |  | | Recommendation/Additional Info |
| Is every slide equipped with sides at least 4 inches in height the entire length of  its sliding surface? | Yes | No |  |
| Does every slide have horizontal entrance platform at the top of its steps that is at least 22 inches in length and as wide as its sliding  surface? | Yes | No |  |
| Does the entrance platform have a protective barrier at least 38 inches high? | Yes | No |  |
| Do slides over 4 feet high have ending surfaces that are at least 11 inches long and are essentially  paralleled to the ground? | Yes | No |  |
| Is the height of the exit between 7 and 15 inches above the ground? | Yes | No |  |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
|  | Slides (cont.) | | | |
| Condition | |  | | Recommendation/Additional Info |
| Are steps corrugated, grooved, or covered with permanent slip-resistant finish and are greater than 3 inches in depth and 16 inches in width? | | Yes | No |  |
| Do all ladders (except those with rungs for hands and feet) and all stairs have continuous handrails on  both sides? | | Yes | No |  |
| Are all access steps, rungs,  railings and handrails free from entrapment openings? | | Yes | No |  |
| Do transition areas and hardware not create entanglement or protrusion hazards? | | Yes | No |  |