Person(s) Conducting the Survey:

Location:

Date:

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
|  | Play Area Layout and Grounds | | | |
| Condition | |  | | Recommendation/Additional Info |
| Is exercise equipment separated from play equipment? | | Yes | No |  |
| Is the equipment  recommended by CPSC? | | Yes | No |  |
| Is the play area free of tripping hazards? | | Yes | No |  |
| Does the play area have proper drainage? | | Yes | No |  |
| Is the area fenced from risks (e.g. parking, streets)? | | Yes | No |  |
| Does each piece of equipment have its own 6-  foot fall zone on all sides? | | Yes | No |  |
| Does each swing have a full fall zone equal to double the length of the swing front and back? | | Yes | No |  |
| Are moving equipment and passive activities separated  from each other? | | Yes | No |  |
| Are there age appropriate play areas? | | Yes | No |  |
| Are provisions in design, layout provided for clear sight lines and supervision? | | Yes | No |  |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
|  | Surface and Curbing | | | |
| Condition | |  | | Recommendation/Additional Info |
| Does each piece of equipment have at least 9 inches of shock-absorbing material underneath and 6 feet beyond its outer edges? | | Yes | No |  |
| Are concrete footings below grade 4 inches or more on equipment and play  structures? | | Yes | No |  |
| Is manufactured surface material in place? | | Yes | No |  |
| Are no tripping hazards  created by separate surfaces’ meeting edges? | | Yes | No |  |
| Is there curbing or containment structure on all sides of loose surface  material? | | Yes | No |  |
| Are curbing or containment structures visible and free of hazards and broken areas? | | Yes | No |  |