Person(s) Conducting the Survey:

Location:

Date:

|  |
| --- |
| Merry-Go-Rounds |
| Condition |  | Recommendation/Additional Info |
| Is the merry-go-round free of an up/down motion and does it have a continuous platform 9-12 inches from the surface? (no open centers) | Yes | No |  |
| Do handrails not protrude beyond the outer edge of the base and is the maximum radius differenceless than 2 inches? | Yes | No |  |
| Is the platform free of spaces or openings .3 inches in diameter? (finger/string entanglement areas) | Yes | No |  |

|  |
| --- |
| Other Playground Hazards |
| Condition |  | Recommendation/Additional Info |
| Are cables, wires, and ropes visible and located out of the traffic flow? | Yes | No |  |
| Is the equipment free of excessive rust, dry rot, orother wood deterioration? | Yes | No |  |
| Is the play area free of excessive litter, broken glass, sharps? | Yes | No |  |

|  |  |
| --- | --- |
|  | Other Playground Hazards (cont.) |
| Condition |  | Recommendation/Additional Info |
| Are basketball nets made of fabric material and in good condition? (no metal nets) | Yes No |  |
| Are basketball and tetherball poles painted a luminous or contrastingcolor? | Yes No |  |