Person(s) Conducting the Survey:

Location:

Date:

|  |  |  |
| --- | --- | --- |
| Condition |  | Recommendation/Additional Info |
| Are fire exit maps near all exit doors? | Yes No |  |
| Is seating in good  condition? | Yes No |  |
| Is auxiliary lighting (battery backup) provided in the event of a power failure? | Yes No |  |
| If overhead (clamp-on style) lighting is used, is each light individually secured with a  safety cable? | Yes No |  |
| Are costumes stored  properly? | Yes No |  |
| Is good general housekeeping maintained in the auditorium? | Yes No |  |
| Are power tools used for set  production? | Yes No |  |
| Do storage areas above stage have proper guardrails, toe boards and  ladder access? | Yes No |  |
| Is proper clearance maintained in front of the electrical panel? (a minimum of 36-inch “clear space”) | Yes No |  |
| Is the stage surface free of  tripping hazards? | Yes No |  |
| Is the fire curtain descent path blocked from sealing to the stage floor? | Yes No |  |

|  |  |  |
| --- | --- | --- |
| Condition |  | Recommendation/Additional Info |
| Is the fire curtain vacuumed every year to removed excess dust? | Yes No |  |
| Is the fire curtain treated with flame retardant chemicals? NFPA 701 Flame Test | Yes No |  |
| Is the stage rigging inspected on a regular basis? | Yes No |  |
| Is the orchestra pit covered  with a pit net? | Yes No |  |